Software for the Advanced Willem Programmer

The latest Version 0.98d5 is below*.

Version 0.98d - Download: Willem98D.zip (643 KB)
Version 0.98d1 - Download: EPROM98D1.zip (803 KB)
Version 0.98d2 - Download: set_up_98d2.exe (844 KB)
Version 0.98d4 - Download: setup_98d4.exe (948 KB)
Version 0.98d5 - Download: setup_98d5_PCB45.exe (952 KB)
Version 0.98c - Download: setup981c.exe (977 KB)

Adds support for the following IC's in addition to those already supported.
Add PIC microchip 14bit
PIC12F629,PIC12F675, PIC16F630, PIC16F676 ,PIC12F635, PIC12F683, PIC16F636, PIC16F684, PIC16F688
PIC16F72/73/74/76/77, PIC16F737/747/767/777,PIC16F87/88,
rfPIC12F675x, PIC16F785/PS200, PIC16F716
Add microchip 14bit,12bit OTP
PIC12C671,PIC12C672,PIC12CE673,PIC12CE674
PIC16C61/71,PIC16C62/64/65/73, PIC16C62A/62B/62C/63/63A/64A/65A/65B/66/67
PIC16C72/72A/73A/74A/74B/76/77, PIC16C620/620A/621/621A/622/622A
PIC16CE/623/624/625, PIC16C710/711/712/716, PIC16C773/774, PIC16C745/765/923/924,PIC16C925/926
PIC16C554/556/557/558, PIC16C432/433, PIC16C717/770/771/781/782
Add PIC microchip 12bit (FLASH memory)
PIC12F508/509, PIC10F200/202/204/206,PIC16F505, PIC16F54/57
Add PIC18Fxxx
PIC18F242,18F248,18F252,18F258,18F442,18F448,16F452,16F458
PIC18F1220,18F2220,18F4220,18F1320,18F2320,18F4320
PIC18F6520,18F6620,18F6720,18F8520,18F8620,18F8720
PIC18F2331,18F2431,18F4331,18F4431
PIC18F6525,18F6621,18F8525,18F8621
PIC18F6585,18F6680,18F8585,18F8680
PIC18F2439,18F2539,18F4439,18F4539
PIC18F6410,18F8410,18F6490,18F8490
Add PIC18Fxxx
PIC18F2410, PIC18F2420, PIC18F2455
PIC18F2510, PIC18F2515, PIC18F2520, PIC18F2525, PIC18F2550, PIC18F2585
PIC18F2610, PIC18F2620, PIC18F2680
PIC18F4410, PIC18F4420, PIC18F4455
PIC18F4510, PIC18F4515, PIC18F4520, PIC18F4525, PIC18F4550, PIC18F4585
PIC18F4610, PIC18F4620, PIC18F4680
Add Find and edit value OSCCAL (PIC12F629/675, PIC16F630/676)
Add Edit config at address 0x2008,0x2009 (PIC12F635/683,PIC16F636/684/688,PIC16F785)
Fixed Programming PIC all
Test on chip
PIC12F675, PIC16F676, PIC16F684 ,PIC16F767, PIC16F74
PIC16F872, PIC16F876, PIC16F877, PIC16F876A, PIC16F873A, PIC16F819
PIC16F84, PIC16F84A, PIC16F628, PIC16F628A,
eprom PIC12C509JW, PIC16C505JW, PIC16C711JW, PIC16CE625JW
PIC18F458, PIC18F4320, PIC18LF258, PIC18F4539, PIC18F4431

Back to EPROM Tools

For PCB3.5 it is recommended that you use Version 0.98c as this will indicate the correct adapters.

For PCB4.5C it is recommended that Version 0.98D5 is used.

##### Please contact our Web Master with questions or comments.
Copyright DarkWire © 2005. All rights reserved.

[Batch Files] [Electronics Books] [Parallel Port] [PCB CAD Software] [PC Books] [Programming] [Serial Port]
[Audio] [Electronic Design] [Essentials] [Miscellaneous] [PC Diagnostics] [Send your Software] [Source Code]